LEAD CLEARANCE EXAMINATION REPORT

	Insert Property Photo (Side A) Here 















PERFORMED AT:
Address
Cleveland, Ohio, Zip
Date of Construction: Year
Permanent Parcel #:
Total Number of Units: 
Total Number of Units Tested:

PROPERTY OWNER INFORMATION:
Owner’s Name
Owner’s Address
City, State, Zip
Phone:
E-Mail:

OPTIONAL RESPONSIBLE PARTY: (i.e. Property Manager)
Name
Address
City, State, Zip
Phone:
E-Mail:

INVESTIGATOR:
Name
License # 
Address
City, State, Zip 
Phone:
E-Mail:


	Investigator Signature:
	



DATE OF ASSESSMENT:
 (As Listed on Laboratory Report):
DATE OF REPORT: 
		
	
DISCLOSURE STATEMENTS

SECTION 5302.30 OF THE OHIO REVISED CODE REQUIRES TRANSFERORS OF RESIDENTIAL REAL PROPERTY BY SALE, LAND INSTALLMENT CONTRACT, LEASE WITH OPTION TO PURCHASE, EXCHANGE, OR LEASE FOR A TERM OF NINETY-NINE YEARS AND RENEWABLE FOREVER, TO COMPLETE AND PROVIDE A COPY TO THE PROSPECTIVE TRANSFEREE OF THE APPLICABLE PROPERTY DISCLOSURE FORMS, DISCLOSING KNOWN HAZARDOUS CONDITIONS OF THE PROPERTY, INCLUDING LEAD-BASED PAINT HAZARDS.

FEDERAL LAW (24 CFR PART 35 AND 40 CFR PART 745) REQUIRES THE SELLERS OR LESSORS OF RESIDENTIAL PROPERTY CONSTRUCTED PRIOR TO 1978, EXCEPT HOUSING FOR THE ELDERLY OR PERSONS WITH DISABILITIES (UNLESS ANY CHILD WHO IS LESS THAN SIX YEARS OLD RESIDES OR IS EXPECTED TO RESIDE IN SUCH HOUSING) OR ANY ZERO-BEDROOM DWELLING, TO DISCLOSE AND PROVIDE A COPY OF THIS REPORT TO NEW PURCHASERS OR LESSEES (TENANTS) BEFORE THEY BECOME OBLIGATED UNDER A LEASE OR SALES CONTRACT. 

PROPERTY OWNERS AND SELLERS ARE ALSO REQUIRED TO DISTRIBUTE AN EDUCATIONAL PAMPHLET APPROVED BY THE UNITED STATES ENVIRONMENTAL PROTECTION AGENCY AND INCLUDE STANDARD WARNING LANGUAGE IN LEASES OR SALES CONTRACTS TO ENSURE PARENTS HAVE THE INFORMATION THEY NEED TO PROTECT CHILDREN FROM LEAD-BASED PAINT HAZARDS.

THERE MAY BE UNIDENTIFIED LEAD PAINT OR LEAD PAINT HAZARDS IN THIS RESIDENCE, DUE TO THE LIMITED NATURE OF A LEAD CLEARANCE REPORT FOLLOWING LIMITED PAINT FILM STABILIZATION WORK. UN-SAMPLED SURFACE DUST MAY BE A LEAD HAZARD. SAMPLED OR UN-SAMPLED PAINT, SOIL, OR DUST WITH LESS THAN REGULATED AMOUNTS OR CONCENTRATIONS OF LEAD MAY CREATE LEAD HAZARDS IF CHEWED, SWALLOWED, INHALED, OR IF THE PAINT IS TURNED INTO DUST OR CHIPS BY ABRASION, SCRAPING, SANDING, OR OTHER DISTURBANCE.
 


	Clearance Investigator:
	
	Date:
	

























PLEASE NOTE: COMPLETE ALL ITEMS IN RED AS APPROPRIATE, DELETE ALL REMAINING COMMENTS IN RED BEFORE SAVING. SUBMIT THE FINAL VERSION OF THIS CLEARANCE REPORT. ENSURE ALL PAGES AND ATTACHMENTS ARE LINED UP PROPERLY.

DESCRIPTION OF PROPERTY & UNIT TYPES (Interior & Exterior):
Describe the subject property to include # of units and unit types, (i.e. 2 story, wood frame structure with 2 rental units).  Describe floor plans, (i.e. efficiency, 1 bedroom, 2 bedroom, etc.). Appurtenant structures such as garages, sheds, porches, etc.

PROPERTY OWNER OCCUPIED:
If Applicable, owner occupied units are exempt from inspection / testing. Identify the unit occupied by the property owner. 

DESCRIPTION OF WORK PERFORMED:
(Describe scope of RRP work, if any). Work was started on date and all work was completed on date. The scope of work included: (i.e. environmental cleaning throughout) 

CONTRACTOR / RRP / LEAD SERVICE PROVIDER INFORMATION:
Property Prepared / Cleaned / Remediated By: N/A (If None Used)
Company name, ODH Certification #:      
Abatement Supervisor Or Renovator Name, ODH Certification #:
Company Street Address
Company City, State, Zip Code
Phone Number
E-Mail Address

VISUAL INSPECTION OF THE EXTERIOR: 
Edit section to describe results of exterior visual inspection. Any deteriorated paint, debris, bare soil, paint chips, etc. is considered an immediate failed lead inspection. No further inspections or testing should occur.
On date, a visual inspection of the exterior found no dust, debris, or paint chips on the ground or on horizontal surfaces in the work areas and adjacent to the work areas. All painted surfaces were in good condition at the time of this clearance examination.

VISUAL INSPECTION OF THE INTERIOR: 
Edit to describe results of interior visual inspection. Any deteriorated paint, dust, debris, paint chips, etc. is considered an immediate failed lead inspection. No further inspections or testing (dust wipe sampling) should occur.

On date, a visual inspection was conducted in the (list rooms visually inspected). No visible dust, debris, or paint chips were observed on floors or any horizontal surfaces. All painted surfaces were in good condition at the time of this clearance examination.

DUST SAMPLE ANALYSIS: 
On date, a total of xx dust wipe samples were collected and analyzed.  One field blank sample anonymously marked was included and analyzed as a quality control check.  Samples were analyzed by:

Dust wipe samples were collected following documented protocol and sampling methodologies found in the U.S. Department of Housing and Urban Development (HUD) “Guidelines for the Evaluation and Control of Lead-Based Paint Hazards in Housing.” Second Edition 2012. The field collection of settled dust samples using wipe sampling methods is used to determine the presence of lead dust hazards on floors, windowsills, and window troughs in a residential structure. In Ohio, a lead dust hazard is present if the laboratory results show levels of lead that are equal to or are greater than 10 micrograms per square foot (µg/ft²) on a floor, 100 µg/ft² on a windowsill, and 100 µg/ft² on a window trough.

LABORATORY INFORMATION:
Laboratory Name
ODH Certification #:      
Street Address
City, State, Zip Code
Phone
E-Mail

FINDINGS (PASSED CLEARANCE): 
Based on the results of a visual inspection and laboratory analysis of dust wipe samples, no lead hazards were identified. Future activities in and around the property may create new lead hazards or cause lead hazards corrected with interim control methods to reappear.  THIS PROPERTY HAS PASSED CLEARANCE.

It is recommended that regular ongoing monitoring and visual inspection of the property be conducted to identify any areas of new deterioration. This may be done by the home owner or a certified risk assessor or hazard investigator. Any area of new deterioration, rot, and substrate or component failure should be corrected with an ongoing property maintenance program.

FINDINGS (FAILED CLEARANCE): 
Based on the results of laboratory analysis of dust wipe samples, lead dust hazards were identified in the (list rooms and components that failed) i.e. kitchen floor, living room carpet, and bedroom 2 window trough. The contractor was notified of the responsibility to re-clean all failed components in the rooms that failed and in all un-sampled rooms.  THIS PROPERTY HAS FAILED CLEARANCE.

On date, a total of xx dust wipe samples were collected from areas that had failed clearance and were analyzed. Re-testing was performed to HUD/ODH guidelines. A minimum of four (4) re-test dust wipe samples of all failed components and like components not previously tested are required. One field blank sample anonymously marked was included and analyzed as a quality control check. 


Cc : Owner 
     :Tenant (If Applicable)
     : Responsible Party (If Applicable)
       

ATTACHMENTS
· Floor Plans With Sample Locations Marked 
· Copy of Lab Results including Chain of Custody forms
· Photos of All 4 Sides of House and Interior work completed.
· ODH Form HEA7730 – Clearance Examination Report 
· ODH Form HEA7731 – Lead Hazard Control Visual Clearance 
· Copies of Licenses and Certifications for all Lead Licensed Service Providers Used on the project.
· Ongoing Lead-Based Paint Maintenance and Reevaluation
· Other Information As Required By The Local Jurisdiction.









ONGOING LEAD-BASED PAINT MAINTENANCE AND REEVALUATION ACTIVITIES (24 CFR § 35.1355)
64 FR 50218, Sept. 15, 1999, as amended at 69 FR 34275, June 21, 2004

(a) Maintenance. Maintenance activities shall be conducted in accordance with paragraphs (a)(2)-(6) of this section, except as provided in paragraph (a)(1) of this section.
(1) Maintenance activities need not be conducted in accordance with this section if a lead-based paint inspection indicates that no lead-based paint is present in the dwelling units, common areas, and on exterior surfaces, or a clearance report prepared in accordance with § 35.1340(a) indicates that all lead-based paint has been removed.
(2) A visual assessment for deteriorated paint, bare soil, and the failure of any hazard reduction measures shall be performed at unit turnover and every twelve months.
(3) (i) Deteriorated paint. All deteriorated paint on interior and exterior surfaces located on the residential property shall be stabilized in accordance with § 35.1330(a)(b), except for any paint that an evaluation has found is not lead-based paint.
(ii) Bare soil. All bare soil shall be treated with standard treatments in accordance with § 35.1335(d) through (g), or interim controls in accordance with § 35.1330(a) and (f); except for any bare soil that a current evaluation has found is not a soil-lead hazard.
(4) Safe work practices, in accordance with sec. 35.1350, shall be used when performing any maintenance or renovation work that disturbs paint that may be lead-based paint.
(5) Any encapsulation or enclosure of lead-based paint or lead-based paint hazards which has failed to maintain its effectiveness shall be repaired, or abatement or interim controls shall be performed in accordance with §§ 35.1325 or 35.1330, respectively.
(6) Clearance testing of the worksite shall be performed at the conclusion of repair, abatement or interim controls in accordance with § 35.1340.
(7) Each dwelling unit shall be provided with written notice asking occupants to report deteriorated paint and, if applicable, failure of encapsulation or enclosure, along with the name, address and telephone number of the person whom occupants should contact. The language of the notice shall be in accordance with § 35.125(c)(3). The designated party shall respond to such report and stabilize the deteriorated paint or repair the encapsulation or enclosure within 30 days.
(b) Reevaluation. Reevaluation shall be conducted in accordance with this paragraph (b), and the designated party shall conduct interim controls of lead-based paint hazards found in the reevaluation.
(1) Reevaluation shall be conducted if hazard reduction has been conducted to reduce lead-based paint hazards found in a risk assessment or if standard treatments have been conducted, except that reevaluation is not required if any of the following cases are met:
(i) An initial risk assessment found no lead-based paint hazards;
(ii) A lead-based paint inspection found no lead-based paint; or
(iii) All lead-based paint was abated in accordance with § 35.1325, provided that no failures of encapsulations or enclosures have been found during visual assessments conducted in accordance with § 35.1355(a)(2) or during other observations by maintenance and repair workers in accordance with § 35.1355(a)(5) since the encapsulations or enclosures were performed.
(2) Reevaluation shall be conducted to identify:
(i) Deteriorated paint surfaces with known or suspected lead-based paint;
(ii) Deteriorated or failed interim controls of lead-based paint hazards or encapsulation or enclosure treatments;
(iii) Dust-lead hazards; and
(iv) Soil that is newly bare, with lead levels equal to or above the standards in § 35.1320(b)(2).
(3) Each reevaluation shall be performed by a certified risk assessor.
(4) Each reevaluation shall be conducted in accordance with the following schedule if a risk assessment or other evaluation has found deteriorated lead-based paint in the residential property, a soil-lead hazard, or a dust-lead hazard on a floor or interior window sill. (Window troughs are not sampled during reevaluation). The first reevaluation shall be conducted no later than two years from completion of hazard reduction. Subsequent reevaluation shall be conducted at intervals of two years, plus or minus 60 days. To be exempt from additional reevaluation, at least two consecutive reevaluations conducted at such two-year intervals must be conducted without finding lead-based paint hazards or a failure of an encapsulation or enclosure. If, however, a reevaluation finds lead-based paint hazards or a failure, at least two more consecutive reevaluations conducted at such two year intervals must be conducted without finding lead-based paint hazards or a failure.
(5) Each reevaluation shall be performed as follows:
(i) Dwelling units and common areas shall be selected and reevaluated in accordance with § 35.1320(b).
(ii) The worksites of previous hazard reduction activities that are similar on the basis of their original lead-based paint hazard and type of treatment shall be grouped. Worksites within such groups shall be selected and reevaluated in accordance with § 35.1320(b).
(6) Each reevaluation shall include reviewing available information, conducting selected visual assessment, recommending responses to hazard reduction omissions or failures, performing selected evaluation of paint, soil and dust, and recommending response to newly-found lead-based paint hazards.
      (i) Review of available information. 
The risk assessor shall review any available past evaluation, hazard reduction and clearance reports, and any other available information describing hazard reduction measures, ongoing maintenance activities, and relevant building operations.
(ii) Visual assessment. The risk assessor shall:
(A) Visually evaluate all lead-based paint hazard reduction treatments, any known or suspected lead-based paint, any deteriorated paint, and each exterior site, and shall identify any new areas of bare soil;
(B) Determine acceptable options for controlling the hazard; and
(C) Await the correction of any hazard reduction omission or failure and the reduction of any lead-based paint hazard before sampling any dust or soil the risk assessor determines may reasonably be associated with such hazard.
(iii) Reaction to hazard reduction omission or failure. 
If any hazard reduction control has not been implemented or is failing (e.g., an encapsulant is peeling away from the wall, a paint-stabilized surface is no longer intact, or gravel covering an area of bare soil has worn away), or deteriorated lead-based paint is present, the risk assessor shall:


(A) Determine acceptable options for controlling the hazard; and
(B) Await the correction of any hazard reduction omission or failure and the reduction of any lead-based paint hazard before sampling any dust or soil the risk assessor determines may reasonably be associated with such hazard.
(iv) Selected paint, soil and dust evaluation.
(A) The risk assessor shall sample deteriorated paint surfaces identified during the visual assessment and have the samples analyzed, in accordance with 40 CFR 745.227(b)(3)(4), but only if reliable information about lead content is unavailable.
(B) The risk assessor shall evaluate new areas of bare soil identified during the visual assessment. Soil samples shall be collected and analyzed in accordance with 40 CFR 745.227(d)(8)-(11), but only if the soil lead levels have not been previously measured.
(C) The risk assessor shall take selected dust samples and have them analyzed. Dust samples shall be collected and analyzed in accordance with § 35.1320(b). At least two composite samples, one from floors and the other from interior window sills, shall be taken in each dwelling unit and common area selected. Each composite sample shall consist of four individual samples, each collected from a different room or area. If the dwelling unit contains both carpeted and uncarpeted living areas, separate floor samples are required from the carpeted and uncarpeted areas. Equivalent single-surface sampling may be used instead of composite sampling.
(7) The risk assessor shall provide the designated party with a written report documenting the presence or absence of lead-based paint hazards, the current status of any hazard reduction and standard treatment measures used previously and any newly-conducted evaluation and hazard reduction activities. The report shall include the information in 40 CFR 745.227(d)(11), and shall:
(i) Identify any lead-based paint hazards previously detected and discuss the effectiveness of any hazard reduction or standard treatment measures used, and list those for which no measures have been used.
(ii) Describe any new hazards found and present the owner with acceptable control options and their accompanying reevaluation schedules.
(iii) Identify when the next reevaluation, if any, must occur, in accordance with the requirements of paragraph (b)(4) of this section.
(c) Response to the reevaluation -
(1) Hazard reduction omission or failure found by a reevaluation. 
The designated party shall respond in accordance with paragraph (b)(6)(iii)(A) of this section to a report by the risk assessor of a hazard reduction control that has not been implemented or is failing, or that deteriorated lead-based paint is present.
(2) Newly-identified lead-based paint hazard found by a reevaluation. 
The designated party shall treat each:
(i) Dust-lead hazard or paint lead hazard by cleaning or hazard reduction measures, which are considered completed when clearance is achieved in accordance with § 35.1340.
(ii) Soil-lead hazard by hazard reduction measures, which are considered completed when clearance is achieved in accordance with § 35.1340.












UNIT DIAGRAMS:
Reproduce as Needed for Additional Floors. Detail windows, doors and sampling locations.
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LABORATORY ANALYSIS REPORTS AND DOCUMENTS: DUST WIPE SAMPLE ANALYTICAL DATA: 
Remove Placeholder Page and Insert Actual Lab Reports and documents. Marked-up or edited laboratory documents will result in deficiency. All edits must be done by laboratory.

· Laboratory Analysis Report For All Dwelling Units Tested
· Laboratory Analysis Report For Any Re-Testing of Failed Samples
· Chain of Custody















































LABORATORY ANALYSIS REPORTS: SOIL SAMPLE ANALYTICAL DATA: 
Must be Done By A Lead Risk Assessor. Clearance Technicians can Identify Bare Soil Only. Remove Placeholder Page and Insert Actual Lab Report.

· Soil Testing Analysis Report 
· Chain of Custody. 
· All Supporting Laboratory Documents 















































ODH FORM 7730 - CLEARANCE EXAMINATION REPORT:
Complete All Applicable Fields. Remove Placeholder Page and Insert Actual ODH Form 7730.




















































ODH FORM 7731 - LEAD HAZARD CONTROL VISUAL CLEARANCE: 
Complete All Applicable Fields. Populate Room Identifier Column For ALL Rooms Visually Inspected To Include Exterior. Check All Appropriate Boxes. Remove Placeholder Page and Insert Actual ODH Form 7731.



















































PROJECT PHOTOS:
Minimum All 4 Sides of Exterior of Home. DO NOT CROP PHOTOS. Photos of Interior Finishes and Testing Locations are Preferred. Remove Placeholder Page and Insert project photos.
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	LEAD CLEARANCE EXAMINATION REPORT

	City of Cleveland
Justin M. Bibb, Mayor
Department of Building and Housing
Division of Record Administration
601 Lakeside Avenue E., Rm. 517
Cleveland, Ohio 44114
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COPY OF LEAD SERVICE PROVIDERS LICENSES & CERTIFICATIONS:
All Licensed Certified / Individuals Working On Project.  Remove Placeholder Page and Insert Copies of Certifications and Licenses.


















































image1.png




